**R63 LED BULB**

**ITEM NO: VT-1862; WATTS:8W**

 

|  |  |
| --- | --- |
| Item No: | VT-1862 |
| SKU Codes | **4221:3000K** |
| Type: | **R63** |
| Base | **E27** |
| Real Watts | **8W** |
| EQ. Watts | **60W** |
| Voltage | **170-240V,50Hz** |
| Input Current | **63ma** |
| Input Efficiency | **62lm/w** |
| Lumen(lm) | **500lm** |
| PF | **>0.5** |
| CRI | **>80** |
| Color Temperature | **3000K,4500K,6000K** |
| Beam Angle | **120’D** |
| LED Chip | **SMD 2835** |
| LED Qty | **16** |
| Driver | **RC Buck** |
| Protection Class | **IP20** |
| Body Material | **Plastic** |
| Dimmable | **No** |
| Unit size | **63\*100mm** |
| Life Time | **20000hrs** |
| Operation Temperature | **-25 ~50’C** |
| Applicable Environment | **Indoor Lighting, Used in Home down light, Stairwell lighting.** |

**Instruction Manual：**

**Installing please following below steps:**

1. **Please note to cut off the power supply before replacing the lamp to prevent electric shock or lamp burning, choose to install to correspondingly lamp holders**
2. **When try to tighten or take off the bulb, please clench radiator body by finger as shown below :**



1. **When need to take off the bulb ,please wait 20minutes after turning off, so as not to burn your fingers**