**LED SURFACE PANEL LIGHTS**

**ITEM NO.: VT- 1408 SQ, WATTS: 8W**

****

|  |  |
| --- | --- |
| Item No: | VT-1408 SQ |
| SKU Code | **4800:6000K (White)** |
| Shape | **Square** |
| Real Watts | **8W** |
| EQ. Watts | **24W** |
| Voltage | **110~265V** |
| Input Frequency | **50/60Hz** |
| Input Efficiency | **60lm/w** |
| Lumen(lm) | **480lm** |
| PF | **>0.9** |
| RA | **>80** |
| Color Temperature | **3000K,4500K,6000K** |
| Beam Angle | **120’D** |
| LED Chip | **SMD 5630** |
| Protection Class | **IP20** |
| Color of Fixture | **Powder Coating Die cast (PKW)**  |
| Body Material | **Aluminum** |
| Dimmable | **No** |
| Unit size | **115\*115mm;H35mm** |
| Cutting size | **70mm\*70mm** |
| Life Time | **20,000hrs** |
| Operation Temperature | **-25 ~50’C** |
| Applicable Environment | **Indoor Lighting, Used in Home down light, Stairwell lighting.** |