**LED PANEL LIGHTS**

**ITEM NO: VT-1209RD; WATTS: 12W**

****

|  |  |
| --- | --- |
| Item No: | VT-1209RD |
| SKU Code | **4879:4500K** |
| Shape | **Round** |
| Real Watts | **12W** |
| EQ. Watts | **48W** |
| Voltage | **DC: 30-42V, Driver:300mA** |
| Input Frequency | **50Hz** |
| Input Efficiency | **75lm/w** |
| Lumen(lm) | **900lm** |
| PF | **>0.7** |
| RA | **>75** |
| Color Temperature | **3000K,4500K,6000K** |
| Beam Angle | **120’D** |
| Color of Fixture | **Powder Coating Die cast (PKW)** |
| Protection Class | **IP20** |
| Body Material | **Plastic** |
| Dimmable | **No** |
| Unit size | **D:170mm;Height:25mm** |
| Cutting Size | **D:155mm** |
| Life Time | **20000hrs** |
| Operation Temperature | **-25 ~50’C** |
| Applicable Environment | **Indoor Lighting, Used in Home down light** |